
(rules PCB cpu-scmp
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (eu.mihosoft.freerouting.autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 13469)
    (layer_rule F.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.8)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.5)
    )
  )
  (rule
    (width 400.0)
    (clear 200.2)
    (clear 125.0 (type smd_to_turn_gap))
    (clear 50.0 (type smd_smd))
  )
  (padstack "Via[0-1]_800:400_um"
    (shape
      (circle F.Cu 800.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 800.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_800:400_um" "Via[0-1]_800:400_um" default
  )
  (via 
    "Via[0-1]_800:400_um-kicad_default" "Via[0-1]_800:400_um" "kicad_default"
  )
  (via_rule
    default "Via[0-1]_800:400_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_800:400_um-kicad_default"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 400.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    "Net-(C12-Pad1)" "Net-(C12-Pad2)" "Net-(C16-Pad1)" "Net-(C16-Pad2)" "Net-(C17-Pad2)" "Net-(C18-Pad1)" "Net-(D1-Pad1)" "Net-(D1-Pad2)"
    "Net-(J1-Pad1)" "Net-(J1-Pad2)" "Net-(J1-Pad3)" "/NKC_D0" "/NKC_D1" "/NKC_D2" "/NKC_D3" "/NKC_D4"
    "/NKC_D5" "/NKC_D6" "/NKC_D7" "/~NKC_RD~" "/~NKC_WR~" "/~NKC_IORQ~" "/~NKC_MREQ~" "/NKC_A0"
    "/NKC_A1" "/NKC_A2" "/NKC_A3" "/NKC_A4" "/NKC_A5" "/NKC_A6" "/NKC_A7" "/~NKC_RESET~"
    "Net-(J1-Pad29)" /CLK "Net-(J1-Pad31)" "/~NKC_INT~" "/~NKC_WAIT~" "/NKC_A8" "/NKC_A9" "/NKC_A10"
    "/NKC_A11" "/NKC_A12" "/NKC_A13" "/NKC_A14" "/NKC_A15" "Net-(J1-Pad42)" "/~NKC_BUSRQ~" "/~NKC_BUSAK~"
    "Net-(J1-Pad45)" "Net-(J1-Pad46)" "Net-(J1-Pad47)" "Net-(J1-Pad48)" "Net-(J1-Pad49)" "Net-(J1-Pad50)" "Net-(J1-Pad51)" "Net-(J1-Pad54)"
    "Net-(J2-Pad10)" "Net-(J2-Pad12)" "Net-(J2-Pad14)" "Net-(J2-Pad16)" "Net-(C10-Pad2)" "Net-(J4-Pad1)" "Net-(J4-Pad2)" "Net-(J4-Pad4)"
    "Net-(J5-Pad1)" "Net-(J5-Pad2)" "Net-(J5-Pad4)" "Net-(JP1-Pad1)" "Net-(JP1-Pad3)" "Net-(JP2-Pad2)" "Net-(C5-Pad2)" "Net-(C7-Pad1)"
    "/FLAG-2" "Net-(Q1-Pad2)" /~NBREQ~ /~NRDS~ /~NWDS~ "Net-(RN2-Pad8)" "Net-(RN2-Pad9)" /D7
    /D6 /D5 /D4 /D3 /D2 /D1 /D0 /~NENIN~
    /A3 /A2 /A1 /A0 /~MREQ~ /~IORQ~ /A7 /A6
    /A5 /A4 /A15 /A14 /A13 /A12 /A11 /A10
    /A9 /A8 "/FLAG-0" "/SENSE-A" "Net-(U13-Pad11)" /~IOADDR~ "Net-(U5-Pad10)" "Net-(U5-Pad4)"
    "Net-(U11-Pad4)" /ADDRVALID "Net-(U6-Pad6)" /ADDRINVALID "/FLAG-1" /SOUT "Net-(U7-Pad4)" /SIN
    "/SENSE-B" "Net-(U7-Pad38)" /~NADS~ "Net-(U8-Pad1)" "Net-(C10-Pad1)" "Net-(U8-Pad8)" "Net-(U10-Pad11)" "Net-(U11-Pad9)"
    "Net-(U14-Pad6)" "Net-(C14-Pad1)" "Net-(X1-Pad1)" "Net-(J2-Pad2)" "Net-(J2-Pad4)" "Net-(J2-Pad6)" "Net-(J2-Pad8)" "Net-(C5-Pad1)"
    "Net-(L1-Pad1)" "Net-(U4-Pad15)" "Net-(U4-Pad16)" "Net-(U4-Pad17)" "Net-(U4-Pad18)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 400.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class pwr
    VCC GND
    (clearance_class default)
    (via_rule default)
    (rule
      (width 800.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)